* Displacement is an important parameter in engineering analysis
* GNSS-based displacement identification and extraction is affected by noise
* GNSS-based displacement detection using Bayesian inference
* Bayesian inference is implemented by Markov Chain Monte Carlo sampling
* Displacement detection is achieved by posterior samples of parameters